> 0 | Document History

> New document: Upgrading Firmware, Version 07
> Preceding document: AN 16: Upgrading Firmware, Version 06

> Chapter | What is new
> 1, 2 | Added Windows Vista.
> 1.4 | Disable power saving before starting the firmware download. Firmware download requires AT+CFUN=1.
> 2.7 | Product specific notes removed.
> 3.2.1 | Avoid autobauding. Choose a fixed baud rate before starting the firmware download.

> New document: Upgrading Firmware, Version 06
> Preceding document: AN 16: Upgrading Firmware on MC75, TC6x, AC75, Version 05

> Chapter | What is new
> Throughout document | Added new products: XT65, XT75. Changed document name and ID.

> New document: Upgrading Firmware, Version 05
> Preceding document: AN 16: Upgrading Firmware on MC75, TC6x, AC75, Version 04

> Chapter | What is new
> Throughout document | Added new product: AC65.

> New document: AN 16, "Upgrading Firmware on MC75, TC6x, AC75", Version 04
> Preceding document: AN 16, " Upgrading Firmware on MC75, TC6x, AC75", Version 03

> Chapter | What is new
> 4.1 | Changed capacitor for IGT-DTR connection (now 4.7µF) in Figure 10.

> New document: AN 16, "Upgrading Firmware on MC75, TC6x, AC75", Version 03
> Preceding document: AN 16, " Upgrading Firmware on MC75, TC6x, AC75", Version 02

> Chapter | What is new
> 1.4 | Shortened description as requirements are detailed in sections 1.4 ‑ 2.7 and 3.3.
> 1.4 ‑ 2.7 | Enhanced all sections, added new sections to describe differences depending on connection between IGT and DTR. Added further details on baudrate settings.

> New document: AN 16, "Upgrading Firmware on MC75, TC6x, AC75", Version 02
> Preceding document: AN 16, " Upgrading Firmware on MC75, TC6x, AC75", Version 01

> Chapter | What is new
> Throughout document | Complete revision because document relates only to gWinSwup and Generic Update. Deleted description of other download programs. Added AC75.