> 8.9 | OTAP Tracer

> For easy debugging of the OTAP scenario, the OTAP procedure can be traced over the serial interface. The trace output shows details of the OTAP procedure and the used parameters. To enable the OTAP trace output use the AT command AT^SCFG, e.g.
> AT^SCFG=Trace/Syslog/OTAP,1
> The serial interface on which you issue this command is then exclusively used for the OTAP tracer. All other functionality which is normally present (AT commands or CommConnection and System.out in Java) is not available when the tracer is on.
> This feature is intended to be used during development phase and not in deployed devices.