> 12.4.3 | Send Java Security Command to the Module

> Use a terminal program. Enter:
> AT^SJSEC
> Wait for the answer:
> CONNECT
> JSEC READY: SEND COMMAND ...
> Now you can send the binary data of the command (for example: from a file with the binary data of the command).
> The module’s answer depends on the result of the operation.
> The read command, AT^SJSEC?, can be used to request the current Java security status.

> Read command AT^SJSEC? | The read command can be used to request the current status of java security. Response ^SJSEC:<state>,<HTTPS state>,<OBEX state>,<untrusted domain> [<certificate content>] <state> Java security mode 0 Unsecured mode, i.e. security mode not active (default) 1 Secured mode, i.e. security mode active <HTTPS state> 0 The HTTPS connection or Secure Connection is possible if the server certificate (or certificate chain) is valid (default) 1 The HTTPS Connection or Secure Connection is possible only if the server certificate is signed by the customer (owner of root certificate in device) <OBEX state> 0 Start of Module Exchange Suite is not permitted 1 Start of Module Exchange Suite is permitted (default) <untrusted domain> 0 Untrusted domain does not exist, MIDlets must be signed (default) 1 Untrusted domain does exist, unsigned MIDlets have limited rights of access to the Java-API Certificate Information: (default no certificate) Issuer: SerialNumber: Subject: Signature algorithm: Thumbprint algoritm: Thumbprint: