> 10.14.1 | Selecting URC Mode or Polling Mode

> To enable or disable the presentation of URCs for the Internet services use the AT^SCFG command, type "TcpIp/WithURCs" and select "on" or "off" for parameter <tcpWithUrc>.

> at^scfg=tcp/withurcs | Query the current setting.
> ^SCFG: "Tcp/WithURCs","on" | URC mode is enabled (delivery detault).
> OK
> at^scfg=tcp/withurcs,off | Select polling mode (by switching off URC mode).
> ^SCFG: "Tcp/WithURCs","off" | Polling mode is accepted.
> OK