> 10.14.7 | Configuring and Using FTP Download (URC Mode)

> First set up a connection profile as explained in Section 10.1.1 or Section 10.1.2. Enter at least all parameters which are mandatory for the connection profile.
> Configure the service profile 1 for FTP:

> at^siss=1,srvType,ftp | Select service type FTP.
> OK
> at^siss=1,conId,0 | Select connection profile 0.
> OK
> at^siss=1,address,"ftp://192.168.1.2;type=d" | Specify FTP address with user and password anonymous.
> OK

> Make an FTP connection:

> at^siso=1 | Open the service.
> OK | Bearer is established, service is getting started.
> ^SISR: 1, 1 | Data is available.
> at^sisr=1,1500 | Request to read 1500 bytes.
> ^SISR: 1, 50 | 50 bytes are now available.
> hardware
> inttest
> software
> support
> systemtest
> OK
> ^SISR: 1, 2 | Data transfer finished. No more data available. The connection to the FTP server is closed.
> at^sisc=1 | Close the service.
> OK