> 0 | Document History

> Preceding document: "TC65 Terminal Hardware Interface Description" Version 02.000b
> New document: "TC65 Terminal Hardware Interface Description" Version 03.000

> Chapter | What is new
> 2.1 | Updated key feature list.
> 2.2 | Added support for Microsoft® Vista™.
> 3.5.5 | Modified startup states for IO6 and IO7.
> 5.2 | ON/OFF line should not be permanently set to active low.
> 5.11 | Updated ADC accuracy values.
> 6.2 | Updated section.
> 7 | Updated Siemens ordering number for TC65 Terminal.

> Preceding document: "TC65 Terminal Hardware Interface Description" Version 02.000a
> New document: "TC65 Terminal Hardware Interface Description" Version 02.000b

> Chapter | What is new
> 1.3.1 | Added MII standards to list of directives and standards (Table 5 and Table 6).

> Preceding document: "TC65 Terminal Hardware Interface Description" Version 01.041
> New document: "TC65 Terminal Hardware Interface Description" Version 02.000a

> Chapter | What is new
> 1.33 | Added automotive directive and CE logo. Updated list of standards.
> 2 | Updated audio features.
> 3.5.5 | New chapter Signal States after Startup
> 3.10; 3.10.1 | Corrected description of IO interface connector pin 7 and pin 8. Added remark on connecting pull-up or pull-down resistors to all GPIO pins used as output.
> 3.10.6 | Removed possibility to backup RTC from a chargeable external battery.
> 5.1 | Changed unit for current consumption in Power Down Mode from μA to mA.
> 5.6 | Modified MICP, MICN characteristics.
> 5.12 | Table 38: Modified RTC input voltage values (RTC backup).

> Preceding document: "TC65 Terminal Hardware Interface Description" Version 01.030
> New document: "TC65 Terminal Hardware Interface Description" Version 01.041

> Chapter | What is new
> Throughout manual | Changed release number; no further changes