> 10.2.1 | Checking Connection Profile Status

> at^sici? | Query the current status of the connection profile.
> ^SICI: 1,2,1,"10.10.0.161" | One connection profile has been created at <conProfileId>=1, and one service is opened using this connection profile. The Internet connection is in <conState>=2 ("Up").
> OK

> Assume the network connection is temporarily not available. (If URC presentation mode of network registration is enabled the state is shown by the URC "+CREG: 2").

> at^sici? | Query once again the current status of the connection profile.
> ^SICI: 1,3,1,"10.10.0.161" | Parameter <conState> has changed to state "Limited up".
> OK

> The network connection is temporarily not available but the Internet connection is still established, so the host may decide to stop the data transfer to minimize the risk of losing data due to memory limitations.

> at^sici? | Query once again the current status of the connection profile.
> ^SICI: 1,2,1,"10.10.0.161" | After re-establishing the network connection, <conState> reverts to state "Up".
> OK

> After closing the service with AT^SISC:

> at^sici? | Query once again the current status of the connection profile.
> ^SICI: 1,2,0,"10.10.0.161" | Parameter <numServices> has decreased. The bearer is still open because the service was closed before expiry of the inactivity timeout "inactTO" of AT^SICS.
> OK
> at^sici? | Query again the current status.
> ^SICI: 1,0,0,"0.0.0.0" | The inactivity timeout "inactTO" of AT^SICS has expired, therefore the bearer is closed now.
> OK