> 23.3 | Available AT Commands and Dependency on SIM PIN

> ø ... Command not available
> - ... Command does not require PIN1
> + ... Command requires PIN1
> ± ... Command sometimes requires PIN1

> Table 23.5: | Available AT Commands and Dependency on SIM PIN

> AT Command | Exec | Test | Read | Write
> Configuration Commands
> AT&F | - | ø | ø | ø
> AT&V | - | ø | ø | ø
> AT&W | - | ø | ø | ø
> ATQ | - | ø | ø | ø
> ATV | - | ø | ø | ø
> ATX | - | ø | ø | ø
> AT\V | - | ø | ø | ø
> ATZ | - | ø | ø | ø
> AT+CFUN | ø | - | - | -
> AT^SMSO | - | - | ø | ø
> AT+GCAP | - | - | ø | ø
> AT+CMEE | ø | - | - | -
> AT+CSCS | ø | - | - | -
> AT^SCFG | ø | - | - | -
> AT^SM20 | ø | - | - | -
> Status Control Commands
> AT+CMER | ø | - | - | -
> AT+CIND | ø | - | - | -
> AT^SIND | ø | - | - | -
> AT+CEER | + | + | ø | ø
> ATS18 | ø | ø | - | -
> AT+CPAS | - | - | ø | ø
> AT+WS46 | ø | - | - | -
> Serial Interface Control Commands
> AT\Q | - | ø | ø | ø
> AT&C | - | ø | ø | ø
> AT&D | - | ø | ø | ø
> AT&S | - | ø | ø | ø
> ATE | - | ø | ø | ø
> AT+ICF | ø | - | - | -
> AT+IFC | ø | - | - | -
> AT+ILRR | ø | + | + | +
> AT+IPR | ø | - | - | -
> AT+CMUX | ø | - | - | -
> AT^STPB | ø | - | - | -
> Security Commands
> AT+CPIN | ø | - | - | -
> AT+CPIN2 | ø | + | + | +
> AT^SPIC | - | - | - | -
> AT+CLCK | ø | + | ø | +
> AT^SLCK | ø | + | ø | +
> AT+CPWD | ø | + | ø | +
> AT^SPWD | ø | ± | ø | ±
> AT^SCSL | ø | - | ø | -
> Identification Commands
> ATI | - | ø | ø | ø
> AT+CGMI | - | - | ø | ø
> AT+GMI | - | - | ø | ø
> AT+CGMM | - | - | ø | ø
> AT+GMM | - | - | ø | ø
> AT+CGMR | - | - | ø | ø
> AT+GMR | - | - | ø | ø
> AT+CGSN | - | - | ø | ø
> AT+GSN | - | - | ø | ø
> AT+CIMI | + | + | ø | ø
> Call related Commands
> ATA | + | ø | ø | ø
> ATD | ± | ø | ø | ø
> ATD><mem><n> | + | ø | ø | ø
> ATD><n> | + | ø | ø | ø
> ATD><str> | + | ø | ø | ø
> ATDI | + | ø | ø | ø
> ATDL | + | ø | ø | ø
> ATH | - | ø | ø | ø
> AT+CHUP | + | + | ø | ø
> AT^SHUP | ø | + | ø | +
> ATS0 | ø | ø | - | +
> ATS6 | ø | ø | - | -
> ATS7 | ø | ø | - | -
> ATS8 | ø | ø | - | -
> ATS10 | ø | ø | - | -
> ATO | - | ø | ø | ø
> +++ | - | ø | ø | ø
> AT+CBST | ø | - | - | -
> AT+CRLP | ø | - | - | -
> AT+CLCC | + | + | ø | ø
> AT^SLCC | + | + | + | +
> AT+CR | ø | + | + | +
> AT+CRC | ø | - | - | -
> AT+CSNS | ø | - | - | -
> AT^SCNI | + | + | ø | ø
> AT^SLCD | + | + | ø | ø
> AT^STCD | + | + | ø | ø
> ATP | - | ø | ø | ø
> ATT | - | ø | ø | ø
> Network Service Commands
> AT+COPN | + | + | ø | ø
> AT+COPS | ø | - | ± | ±
> AT^SOPS | ø | + | ø | ø
> AT^SNWS | ø | + | ø | +
> AT+CREG | ø | - | - | -
> AT+CSQ | - | - | ø | ø
> AT^SMONC | + | + | ø | ø
> AT^SMOND | + | + | ø | ø
> AT^SFNUR | ø | - | - | -
> AT^MONI | - | - | ø | -
> AT^MONP | - | - | ø | -
> AT^SMONG | + | + | ø | +
> AT^SALS | ø | + | + | +
> AT^SHOM | + | + | ø | ø
> AT^SPLM | + | + | + | +
> AT+CPOL | ø | + | + | +
> AT^SPLR | ø | + | ø | +
> AT^SPLW | ø | + | ø | +
> Supplementary Service Commands
> AT+CACM | ø | + | + | +
> AT^SACM | + | + | ø | +
> AT+CAMM | ø | + | + | +
> AT+CAOC | + | + | + | +
> AT+CCUG | ø | + | + | +
> AT+CCFC | ø | + | ø | +
> AT+CCWA | ø | + | + | +
> AT+CHLD | ø | + | ø | +
> AT+CLIP | ø | - | + | -
> AT+CLIR | ø | + | + | +
> AT+COLP | ø | + | + | +
> AT+CPUC | ø | + | + | +
> AT+CSSN | ø | - | - | -
> AT+CUSD | ø | + | + | +
> Internet Service Commands
> AT^SICS | ø | - | - | -
> AT^SICI | ø | - | - | -
> AT^SISS | ø | - | - | -
> AT^SISI | ø | - | - | -
> AT^SISO | ø | - | - | +
> AT^SISC | ø | - | ø | +
> AT^SISR | ø | - | ø | +
> AT^SISW | ø | - | ø | +
> AT^SICO | ø | + | + | +
> AT^SICC | ø | + | ø | +
> AT^SISX | ø | + | ø | +
> AT^SISE | ø | - | ø | -
> GPRS Commands
> AT+CGACT | ø | + | + | +
> AT+CGANS | ø | + | ø | +
> AT+CGATT | ø | + | + | +
> AT+CGAUTO | ø | + | + | +
> AT+CGDATA | ø | + | ø | +
> AT+CGDCONT | ø | + | + | +
> AT+CGEQMIN | ø | + | + | +
> AT+CGEQREQ | ø | + | + | +
> AT+CGPADDR | ø | + | ø | +
> AT+CGQMIN | ø | + | + | +
> AT+CGQREQ | ø | + | + | +
> AT+CGREG | ø | + | + | +
> AT+CGSMS | ø | + | + | +
> AT^SGACT | + | + | + | ø
> AT^SGAUTH | ø | - | - | -
> AT^SGCONF | ø | - | - | -
> ATA | + | ø | ø | ø
> ATD*99# | + | ø | ø | ø
> ATD*98# | + | ø | ø | ø
> ATH | + | ø | ø | ø
> ATS0 | ø | ø | - | +
> FAX Commands
> AT+FCLASS | ø | - | - | -
> AT+FRH | ø | - | ø | -
> AT+FRM | ø | - | ø | -
> AT+FRS | ø | ø | ø | -
> AT+FTH | ø | - | ø | -
> AT+FTM | ø | - | ø | -
> AT+FTS | ø | ø | ø | -
> Short Message Service (SMS) Commands
> AT+CMGC | ø | + | ø | +
> AT+CMGD | ø | + | ø | +
> AT+CMGF | ø | - | - | -
> AT+CMGL | + | + | ø | +
> AT+CMGR | ø | + | ø | +
> AT+CMGS | ø | + | ø | +
> AT+CMGW | + | + | ø | +
> AT+CMSS | ø | + | ø | +
> AT+CNMA | + | + | ø | +
> AT+CNMI | ø | + | + | +
> AT+CPMS | ø | + | + | +
> AT+CSCA | ø | + | + | +
> AT+CSCB | ø | + | + | +
> AT+CSDH | ø | + | + | +
> AT+CSMP | ø | + | + | +
> AT+CSMS | ø | + | + | +
> AT^SCML | + | + | ø | +
> AT^SCMR | ø | + | ø | +
> AT^SCMS | ø | + | ø | +
> AT^SCMW | ø | + | ø | +
> AT^SLMS | + | + | ø | ø
> AT^SMGL | + | + | ø | +
> AT^SMGO | ø | + | + | +
> AT^SMGR | ø | + | ø | +
> AT^SSCONF | ø | - | - | -
> AT^SSDA | ø | - | - | -
> AT^SSMSS | ø | + | + | +
> SIM related Commands
> AT+CRSM | ø | ± | ø | ±
> AT+CSIM | ø | - | ø | -
> AT^SATR | - | - | ø | ø
> AT^SXSM | ø | + | ø | +
> AT^SCKS | ø | - | - | -
> AT^SSET | ø | - | - | -
> AT^SCID | - | - | ø | ø
> AT+CXXCID | - | - | ø | ø
> Remote SIM Access (RSA) Commands
> AT^SRSA | ø | - | - | -
> AT^SRSM | ø | - | ø | -
> SIM Application Toolkit (SAT) Commands
> AT^SSTA | ø | - | - | -
> ^SSTN | ø | ø | ø | ø
> AT^SSTGI | ø | - | - | -
> AT^SSTR | ø | - | - | -
> Phonebook Commands
> AT+CNUM | + | + | ø | ø
> AT+CPBR | ø | + | ø | +
> AT+CPBS | ø | + | + | +
> AT+CPBW | ø | + | ø | +
> AT^SPBW | ø | + | ø | +
> AT^SDLD | + | + | ø | ø
> AT^SPBC | ø | + | ø | +
> AT^SPBD | ø | + | ø | +
> AT^SPBG | ø | + | ø | +
> AT^SPBS | ø | + | ø | +
> Audio Commands
> ATL | - | ø | ø | ø
> ATM | - | ø | ø | ø
> AT+CLVL | ø | - | - | -
> AT+CMUT | ø | - | - | -
> AT+VTD | ø | - | - | -
> AT+VTS | ø | - | ø | -
> AT^SAIC | ø | - | - | -
> AT^SNFA | ø | - | - | -
> AT^SNFD | - | - | ø | ø
> AT^SNFG | ø | - | ø | -
> AT^SNFI | ø | - | - | -
> AT^SNFM | ø | - | - | -
> AT^SNFO | ø | - | - | -
> AT^SNFPT | ø | - | - | -
> AT^SNFS | ø | - | - | -
> AT^SNFTTY | ø | - | - | -
> AT^SNFV | ø | - | - | -
> AT^SNFW | - | - | ø | ø
> AT^SRTC | - | - | - | -
> Hardware Related Commands
> AT+CCLK | ø | - | - | -
> AT+CALA | ø | - | - | -
> AT^SBC | ø | - | - | -
> AT^SBV | - | - | ø | ø
> AT^SCTM | ø | - | - | -
> AT^SSYNC | ø | - | - | -
> AT^SSPI | ø | - | - | -
> AT^SAADC | ø | ø | - | ø
> AT^SRADC | ø | - | - | -
> AT^SWDAC | ø | - | - | -
> GPIO Commands
> AT^SPIO | ø | - | ø | -
> AT^SCPIN | ø | - | ø | -
> AT^SCPOL | ø | - | ø | -
> AT^SCPORT | ø | - | ø | -
> AT^SDPORT | ø | - | ø | -
> AT^SGIO | ø | - | ø | -
> AT^SSIO | ø | - | ø | -
> AT^SCCNT | ø | - | - | -
> AT^SSCNT | ø | - | - | -
> Java related Commands
> AT^SJRA | ø | - | ø | -
> AT^SJNET | ø | - | - | -
> AT^SJOTAP | - | - | - | -
> AT^SJSEC | - | ø | - | ø
> Miscellaneous Commands
> A/ | - | ø | ø | ø
> ATS3 | ø | ø | - | -
> ATS4 | ø | ø | - | -
> ATS5 | ø | ø | - | -
> AT^SFDL | - | - | ø | -