> 10.10 | AT^SICC Internet Connection Close

> The AT^SICC write command releases a connection opened with AT^SICO and restores the previously set inactivity timeout "inactTO" of the selected connection profile.
> The command returns an error if any services are bound to this profile. Before using the AT^SICC write command be sure that all services were closed with AT^SISC.
> Syntax

> Test Command AT^SICC=?
> Response(s)
> [^SICC:(list of defined <conProfileId>s)]
> OK

> Write Command AT^SICC=<conProfileId>
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> + |  | + | + | + | + | + | + |  |  | - | - | -

> Parameter Description

> <conProfileId>(num)

> 0...5
> Internet connection profile identifier defined with parameter <conProfileId> of AT^SICS.
> Note

> • | Be sure not to mix up the start and close commands connection profiles and service profiles. It is allowed to use only the combinations AT^SICO / AT^SICC or AT^SISO / AT^SISC.