> 8.2 | Compliance with FCC Rules and Regulations

> The Equipment Authorization Certification for the Siemens reference application described in Section 8.1 will be registered under the following identifiers:
> FCC Identifier: QIPTC65
> Industry Canada Certification Number: 267W-TC65
> Granted to Siemens AG
> Manufacturers of mobile or fixed devices incorporating TC65 modules are authorized to use the FCC Grants and Industry Canada Certificates of the TC65 modules for their own final products according to the conditions referenced in these documents. In this case, the FCC label of the module shall be visible from the outside, or the host device shall bear a second label stating "Contains FCC ID QIP TC65".
> IMPORTANT:
> Manufacturers of portable applications incorporating TC65 modules are required to have their final product certified and apply for their own FCC Grant and Industry Canada Certificate related to the specific portable mobile. This is mandatory to meet the SAR requirements for portable mobiles (see Section 1.3.2 for detail).
> Changes or modifications not expressly approved by the party responsible for compliance could void the user's authority to operate the equipment.
> If the final product is not approved for use in U.S. territories the application manufacturer shall take care that the 850 MHz and 1900 MHz frequency bands be deactivated and that band settings be inaccessible to end users. If these demands are not met (e.g. if the AT interface is accessible to end users), it is the responsibility of the application manufacturer to always ensure that the application be FCC approved regardless of the country it is marketed in. The frequency bands can be set using the command
> AT^SCFG="Radio/Band"[,<rbp>][, <rba>].
> A detailed command description can be found in [1].