> 3.6 | SMTK Uninstall

> The SMTK install package comes with an uninstall facility. The entire SMTK or parts of the package can be removed. To start the uninstall facility, open the Control Panel, select Add/Remove Programs, select the desired SMTK, e.g. TC65 Software Development Kit and follow the instructions. The standard modem and Dial-Up Network connection (DUN) are uninstalled automatically, if no SMTK IMP-NG product is installed in parallel. The user will be asked for uninstall of standard modem and Dial-Up Network (DUN) in the case, that another SMTK IMP-NG product is installed.
> The Module Exchange Suite (MES) is not uninstalled automatically with the SMTK. If you would like to uninstall the Module Exchange Suite (MES) as well, please run the MES uninstall facility. To run the uninstall program, open the Control Panel, select Add/Remove Programs, select Siemens Module Exchange Suite (MES) and follow the instructions.
> Please keep in mind, that standard modem (or USB modem), Dial-Up Network connection and Module Exchange Suite (MES) are required for a proper work of SMTK on-device debugging.
> Note for customers migrating from TC45 to TC65:
> If you uninstall the TC45 software after the installation of TC65 you need to run the TC65 SDK and MES setup in maintenance mode to restore several files required for TC65. To do so, open the Windows Control Panel, double-click Add or Remove Programs, select “TC65 Software Development Kit”, press the Change/Remove button and select Repair. In the same manner, reinstall the Siemens Module Exchange Suite (MES)" As an alternative, to avoid this step, remove the TC45 package, before installing TC65 SDK and MES.