> 2.5.4 | Entering PH SIM PUK

> This section comprises the subsections Description, Used AT Commands, Flow Chart, Hints and Example. To move to these subsections please use the Navigation Frame or the appropriate buttons on the toolbar.

> 2.5.4.1 | Description

> This chapter describes how to enter the PH-SIM PUK. The PH-SIM PUK (also referred to as Master Phone Code) is needed after entering a wrong PH-SIM PIN three times.
> You have two ways to enter the Master Phone Code. The flow chart gives an example of both ways and shows what happens when entering a wrong Master Phone Code. After entering a wrong Master Phone Code, you have to wait several minutes before trying the next Master Phone Code. The time to wait is defined by an algorithm explained in [2].

> 2.5.4.2 | Used AT commands

> Command | Explanation
> AT+CPIN | Enter PIN
> ATD*#0003*Master Phone Code#; | Entering Master Phone Code
> AT^SPIC | Display PIN counter

> For further details about the commands see [2].

> 2.5.4.3 | Flow chart

> Figure 21: Entering PH-SIM PUK

> 2.5.4.4 | Hints

> Not applicable.

> 2.5.4.5 | Example

> ***************************************
> Comment: Entering PH-SIM PUK
> ***************************************
> ***************************************
> Comment: Entering wrong PH-SIM PIN 3 times.
> ***************************************
> Subscr 1 Send: AT+CPIN=0815
> Subscr 1 Receive: AT+CPIN=0815
> Subscr 1 Receive:
> Subscr 1 Receive: +CME ERROR: incorrect password
> Subscr 1 Send: AT^SPIC
> Subscr 1 Receive: AT^SPIC
> Subscr 1 Receive: ^SPIC: 2
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> Subscr 1 Send: AT+CPIN=0815
> Subscr 1 Receive: AT+CPIN=0815
> Subscr 1 Receive:
> Subscr 1 Receive: +CME ERROR: incorrect password
> Subscr 1 Send: AT^SPIC
> Subscr 1 Receive: AT^SPIC
> Subscr 1 Receive: ^SPIC: 1
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> Subscr 1 Send: AT+CPIN=0815
> Subscr 1 Receive: AT+CPIN=0815
> Subscr 1 Receive:
> Subscr 1 Receive: +CME ERROR: incorrect password
> Subscr 1 Send: AT^SPIC
> Subscr 1 Receive: AT^SPIC
> Subscr 1 Receive: ^SPIC: 63
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Request required PIN.
> ***************************************
> Subscr 1 Send: AT+CPIN?
> Subscr 1 Receive: AT+CPIN?
> Subscr 1 Receive: +CPIN: PH-SIM PUK
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Request PIN counter.
> ***************************************
> Subscr 1 Send: AT^SPIC
> Subscr 1 Receive: AT^SPIC
> Subscr 1 Receive: ^SPIC: 63
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Entering wrong PH-SIM PUK.
> ***************************************
> Subscr 1 Send: AT+CPIN=12345678
> Subscr 1 Receive: AT+CPIN=12345678
> Subscr 1 Receive:
> Subscr 1 Receive: +CME ERROR: incorrect password
> ***************************************
> Comment: Entering wrong PH-SIM PUK.
> ***************************************
> Subscr 1 Send: AT+CPIN=12345678
> Subscr 1 Receive: AT+CPIN=12345678
> Subscr 1 Receive:
> Subscr 1 Receive: +CME ERROR: incorrect password
> ***************************************
> Comment: Entering wrong PH-SIM PUK.
> ***************************************
> Subscr 1 Send: AT+CPIN=12345678
> Subscr 1 Receive: AT+CPIN=12345678
> Subscr 1 Receive:
> Subscr 1 Receive: +CME ERROR: incorrect password
> ***************************************
> Comment: Entering correct PH-SIM PUK.
> ***************************************
> Subscr 1 Send: AT+CPIN=18424923
> Subscr 1 Receive: AT+CPIN=18424923
> Subscr 1 Receive:
> Subscr 1 Receive: OK