> 2.5.3 | Entering PH SIM PIN

> This section comprises the subsections Description, Used AT Commands, Flow Chart, Hints and Example. To move to these subsections please use the Navigation Frame or the appropriate buttons on the toolbar.

> 2.5.3.1 | Description

> This chapter describes how to enter the PH-SIM PIN. The PH-SIM PIN is needed, if you have locked your ME to a special SIM card (referred to as “PS” lock). You will also see what happens when a wrong PH SIM PIN is entered three times.

> 2.5.3.2 | Used AT commands

> Command | Explanation
> AT+CPIN | Enter PIN
> AT^SPIC | Display PIN counter

> For further details about the commands see [2].

> 2.5.3.3 | Flow chart

> Figure 20: Entering PH-SIM PIN

> 2.5.3.4 | Hints

> Not applicable.

> 2.5.3.5 | Example

> ***************************************
> Comment: Entering PH-SIM PIN
> ***************************************
> ***************************************
> Comment: Request required PIN.
> ***************************************
> Subscr 1 Send: AT+CPIN?
> Subscr 1 Receive: AT+CPIN?
> Subscr 1 Receive: +CPIN: PH-SIM PIN
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Request PIN counter.
> ***************************************
> Subscr 1 Send: AT^SPIC
> Subscr 1 Receive: AT^SPIC
> Subscr 1 Receive: ^SPIC: 3
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Entering wrong PH-SIM PIN first time.
> ***************************************
> Subscr 1 Send: AT+CPIN=5555
> Subscr 1 Receive: AT+CPIN=5555
> Subscr 1 Receive: +CME ERROR: incorrect password
> ***************************************
> Comment: Request PIN counter.
> ***************************************
> Subscr 1 Send: AT^SPIC
> Subscr 1 Receive: AT^SPIC
> Subscr 1 Receive: ^SPIC: 2
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Entering wrong PH-SIM PIN second time.
> ***************************************
> Subscr 1 Send: AT+CPIN=5555
> Subscr 1 Receive: AT+CPIN=5555
> Subscr 1 Receive: +CME ERROR: incorrect password
> ***************************************
> Comment: Request PIN counter.
> ***************************************
> Subscr 1 Send: AT^SPIC
> Subscr 1 Receive: AT^SPIC
> Subscr 1 Receive: ^SPIC: 1
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Entering correct PH-SIM PIN.
> ***************************************
> Subscr 1 Send: AT+CPIN=1234
> Subscr 1 Receive: AT+CPIN=1234
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Request required PIN.
> ***************************************
> Subscr 1 Send: AT+CPIN?
> Subscr 1 Receive: AT+CPIN?
> Subscr 1 Receive: +CPIN: READY
> Subscr 1 Receive:
> Subscr 1 Receive: OK