> 5.10 | GPIO

> The GPIO Java API (classes: InPort, OutPort, InPortListener, StartStopPulseCounter, LimitPulseCounter and LimitPulseCounterListener) is a replacement for the GPIO AT commands (AT^SPIO, AT^SCPIN, ...). Using these classes frees up AT command resources and improves performance. Both APIs can only be used alternatively. Of course the basic system characteristics of a poll interval of 4.6ms (in SLEEP mode up to 2.7s) for pin state change detection does also apply here.
> GPIO Java API is only supported in TC65.