> 23.4 | Availability of AT Commands Depending on Operating Mode of ME

> - ... AT command not supported
> + ... AT command supported
> ± ... AT command partially supported
> See description of AT command for details.

> Table 23.6: | Availability of AT Commands Depending on Operating Mode of ME

> AT Command | Normal Mode | Q | Charge
> Configuration Commands
> AT&F | + | + | -
> AT&V | + | + | -
> AT&W | + | + | -
> ATQ | + | + | -
> ATV | + | + | -
> ATX | + | + | -
> AT\V | + | + | -
> ATZ | + | + | -
> AT+CFUN | + | + | -
> AT^SMSO | + | + | -
> AT+GCAP | + | + | -
> AT+CMEE | + | + | -
> AT+CSCS | + | + | -
> AT^SCFG | + | ± | ±
> AT^SM20 | + | - | -
> Status Control Commands
> AT+CMER | + | + | -
> AT+CIND | + | + | -
> AT^SIND | + | + | -
> AT+CEER | + | + | -
> ATS18 | + | + | -
> AT+CPAS | + | + | -
> AT+WS46 | + | + | -
> Serial Interface Control Commands
> AT\Q | + | + | -
> AT&C | + | + | -
> AT&D | + | + | -
> AT&S | + | + | -
> ATE | + | + | -
> AT+ICF | + | + | -
> AT+IFC | + | + | -
> AT+ILRR | + | + | -
> AT+IPR | + | + | -
> AT+CMUX | + | + | -
> AT^STPB | + | + | -
> Security Commands
> AT+CPIN | + | + | -
> AT+CPIN2 | + | + | -
> AT^SPIC | + | + | -
> AT+CLCK | + | ± | -
> AT^SLCK | + | ± | -
> AT+CPWD | + | ± | -
> AT^SPWD | + | ± | -
> AT^SCSL | + | + | -
> Identification Commands
> ATI | + | + | -
> AT+CGMI | + | + | -
> AT+GMI | + | + | -
> AT+CGMM | + | + | -
> AT+GMM | + | + | -
> AT+CGMR | + | + | -
> AT+GMR | + | + | -
> AT+CGSN | + | + | -
> AT+GSN | + | + | -
> AT+CIMI | + | + | -
> Call related Commands
> ATA | + | - | -
> ATD | + | - | -
> ATD><mem><n> | + | - | -
> ATD><n> | + | - | -
> ATD><str> | + | - | -
> ATDI | + | - | -
> ATDL | + | - | -
> ATH | + | - | -
> AT+CHUP | + | - | -
> AT^SHUP | + | - | -
> ATS0 | + | - | -
> ATS6 | + | + | -
> ATS7 | + | + | -
> ATS8 | + | + | -
> ATS10 | + | + | -
> ATO | + | - | -
> +++ | + | - | -
> AT+CBST | + | + | -
> AT+CRLP | + | + | -
> AT+CLCC | + | - | -
> AT^SLCC | + | - | -
> AT+CR | + | + | -
> AT+CRC | + | + | -
> AT+CSNS | + | + | -
> AT^SCNI | + | - | -
> AT^SLCD | + | + | -
> AT^STCD | + | + | -
> ATP | + | - | -
> ATT | + | - | -
> Network Service Commands
> AT+COPN | + | + | -
> AT+COPS | + | - | -
> AT^SOPS | + | + | -
> AT^SNWS | + | - | -
> AT+CREG | + | - | -
> AT+CSQ | + | - | -
> AT^SMONC | + | - | -
> AT^SMOND | + | - | -
> AT^SFNUR | + | + | -
> AT^MONI | + | - | -
> AT^MONP | + | - | -
> AT^SMONG | + | - | -
> AT^SALS | + | - | -
> AT^SHOM | + | - | -
> AT^SPLM | + | + | -
> AT+CPOL | + | + | -
> AT^SPLR | + | + | -
> AT^SPLW | + | + | -
> Supplementary Service Commands
> AT+CACM | + | + | -
> AT^SACM | + | + | -
> AT+CAMM | + | + | -
> AT+CAOC | + | + | -
> AT+CCUG | + | + | -
> AT+CCFC | + | - | -
> AT+CCWA | + | - | -
> AT+CHLD | + | - | -
> AT+CLIP | + | - | -
> AT+CLIR | + | - | -
> AT+COLP | + | - | -
> AT+CPUC | + | + | -
> AT+CSSN | + | - | -
> AT+CUSD | + | - | -
> Internet Service Commands
> AT^SICS | + | + | -
> AT^SICI | + | + | -
> AT^SISS | + | + | -
> AT^SISI | + | + | -
> AT^SISO | + | - | -
> AT^SISC | + | - | -
> AT^SISR | + | - | -
> AT^SISW | + | - | -
> AT^SICO | + | - | -
> AT^SICC | + | - | -
> AT^SISX | + | - | -
> AT^SISE | + | - | -
> GPRS Commands
> AT+CGACT | + | - | -
> AT+CGANS | + | - | -
> AT+CGATT | + | - | -
> AT+CGAUTO | + | - | -
> AT+CGDATA | + | - | -
> AT+CGDCONT | + | + | -
> AT+CGEQMIN | + | + | -
> AT+CGEQREQ | + | + | -
> AT+CGPADDR | + | + | -
> AT+CGQMIN | + | + | -
> AT+CGQREQ | + | + | -
> AT+CGREG | + | + | -
> AT+CGSMS | + | + | -
> AT^SGACT | + | + | -
> AT^SGAUTH | + | + | -
> AT^SGCONF | + | + | -
> ATA | + | - | -
> ATD*99# | + | - | -
> ATD*98# | + | - | -
> ATH | + | - | -
> ATS0 | + | - | -
> FAX Commands
> AT+FCLASS | + | + | -
> AT+FRH | + | - | -
> AT+FRM | + | - | -
> AT+FRS | + | - | -
> AT+FTH | + | - | -
> AT+FTM | + | - | -
> AT+FTS | + | - | -
> Short Message Service (SMS) Commands
> AT+CMGC | + | - | -
> AT+CMGD | + | + | -
> AT+CMGF | + | + | -
> AT+CMGL | + | + | -
> AT+CMGR | + | + | -
> AT+CMGS | + | - | -
> AT+CMGW | + | + | -
> AT+CMSS | + | - | -
> AT+CNMA | + | - | -
> AT+CNMI | + | + | -
> AT+CPMS | + | + | -
> AT+CSCA | + | + | -
> AT+CSCB | + | + | -
> AT+CSDH | + | + | -
> AT+CSMP | + | + | -
> AT+CSMS | + | + | -
> AT^SCML | + | + | -
> AT^SCMR | + | + | -
> AT^SCMS | + | - | -
> AT^SCMW | + | + | -
> AT^SLMS | + | + | -
> AT^SMGL | + | + | -
> AT^SMGO | + | + | -
> AT^SMGR | + | + | -
> AT^SSCONF | + | + | -
> AT^SSDA | + | + | -
> AT^SSMSS | + | + | -
> SIM related Commands
> AT+CRSM | + | + | -
> AT+CSIM | + | + | -
> AT^SATR | + | + | -
> AT^SXSM | + | + | -
> AT^SCKS | + | + | -
> AT^SSET | + | + | -
> AT^SCID | + | + | -
> AT+CXXCID | + | + | -
> Remote SIM Access (RSA) Commands
> AT^SRSA | + | - | -
> AT^SRSM | + | - | -
> SIM Application Toolkit (SAT) Commands
> AT^SSTA | + | + | -
> ^SSTN | + | + | -
> AT^SSTGI | + | + | -
> AT^SSTR | + | + | -
> Phonebook Commands
> AT+CNUM | + | + | -
> AT+CPBR | + | + | -
> AT+CPBS | + | + | -
> AT+CPBW | + | + | -
> AT^SPBW | + | + | -
> AT^SDLD | + | + | -
> AT^SPBC | + | + | -
> AT^SPBD | + | + | -
> AT^SPBG | + | + | -
> AT^SPBS | + | + | -
> Audio Commands
> ATL | + | + | -
> ATM | + | + | -
> AT+CLVL | + | + | -
> AT+CMUT | + | + | -
> AT+VTD | + | - | -
> AT+VTS | + | - | -
> AT^SAIC | + | + | -
> AT^SNFA | + | + | -
> AT^SNFD | + | + | -
> AT^SNFG | + | + | -
> AT^SNFI | + | + | -
> AT^SNFM | + | + | -
> AT^SNFO | + | + | -
> AT^SNFPT | + | + | -
> AT^SNFS | + | + | -
> AT^SNFTTY | + | - | -
> AT^SNFV | + | + | -
> AT^SNFW | + | + | -
> AT^SRTC | + | + | -
> Hardware Related Commands
> AT+CCLK | + | + | +
> AT+CALA | + | + | +
> AT^SBC | + | + | ±
> AT^SBV | + | + | -
> AT^SCTM | + | + | +
> AT^SSYNC | + | - | -
> AT^SSPI | + | + | -
> AT^SAADC | + | + | -
> AT^SRADC | + | + | -
> AT^SWDAC | + | + | -
> GPIO Commands
> AT^SPIO | + | + | -
> AT^SCPIN | + | + | -
> AT^SCPOL | + | + | -
> AT^SCPORT | + | + | -
> AT^SDPORT | + | + | -
> AT^SGIO | + | + | -
> AT^SSIO | + | + | -
> AT^SCCNT | + | + | -
> AT^SSCNT | + | + | -
> Java related Commands
> AT^SJRA | + | + | -
> AT^SJNET | + | + | -
> AT^SJOTAP | + | - | -
> AT^SJSEC | + | + | -
> Miscellaneous Commands
> A/ | + | + | -
> ATS3 | + | + | -
> ATS4 | + | + | -
> ATS5 | + | + | -
> AT^SFDL | + | + | -