> 23.5 | AT Command Settings storable with AT&W

> Table 23.7: | Settings Stored to User Profile on ASC0 / MUX Channel 1

> AT Command | Stored Parameters
> Configuration Commands
> ATQ | <n>
> ATV | <value>
> ATX | <value>
> AT\V | <value>
> AT+CMEE | <errMode>
> Status Control Commands
> ATS18 | <n>
> Serial Interface Control Commands
> AT\Q | <n>
> AT&C | <value>
> AT&D | <value>
> AT&S | <value>
> ATE | <value>
> AT+ICF | <format>, <parity>
> AT+IFC | <TEflowcontrol>, <TAflowcontrol>
> AT+ILRR | <value>
> AT^STPB | <n>
> Call related Commands
> ATS0 | <n>
> ATS6 | <n>
> ATS7 | <n>
> ATS8 | <n>
> ATS10 | <n>
> AT+CBST | <speed>, <name>, <ce>
> AT+CRLP | <iws>, <mws>, <T1>, <N2>
> AT^SLCC | <n>
> AT+CR | <mode>
> AT+CRC | <mode>
> Network Service Commands
> AT+COPS | <format>
> AT^SNWS | <format>
> AT+CREG | <n>
> Supplementary Service Commands
> AT^SACM | <n>
> AT+CLIP | <n>
> GPRS Commands
> ATS0 | <n>
> FAX Commands
> AT+FCLASS | <n>
> Short Message Service (SMS) Commands
> AT+CMGF | <mode>
> AT+CNMI | <mode>, <mt>, <bm>, <ds>
> AT+CSDH | <show>
> AT+CSMS | <service>
> AT^SMGO | <n>
> SIM related Commands
> AT^SCKS | <mode>
> AT^SSET | <n>
> Miscellaneous Commands
> ATS3 | <n>
> ATS4 | <n>
> ATS5 | <n>

> Table 23.8: | Settings Stored to User Profile on ASC1 / MUX Channels 2 and 3

> AT Command | Stored Parameters
> Configuration Commands
> ATQ | <n>
> ATV | <value>
> ATX | <value>
> AT+CMEE | <errMode>
> Serial Interface Control Commands
> AT\Q | <n>
> AT&C | <value>
> AT&D | <value>
> AT&S | <value>
> ATE | <value>
> AT+ICF | <format>, <parity>
> AT+IFC | <TEflowcontrol>, <TAflowcontrol>
> AT^STPB | <n>
> Call related Commands
> ATS0 | <n>
> AT^SLCC | <n>
> AT+CR | <mode>
> AT+CRC | <mode>
> Network Service Commands
> AT+COPS | <format>
> AT^SNWS | <format>
> AT+CREG | <n>
> Supplementary Service Commands
> AT^SACM | <n>
> AT+CLIP | <n>
> GPRS Commands
> ATS0 | <n>
> Short Message Service (SMS) Commands
> AT+CMGF | <mode>
> AT+CNMI | <mode>, <mt>, <bm>, <ds>
> AT+CSDH | <show>
> AT+CSMS | <service>
> AT^SMGO | <n>
> SIM related Commands
> AT^SCKS | <mode>
> AT^SSET | <n>
> Miscellaneous Commands
> ATS3 | <n>
> ATS4 | <n>
> ATS5 | <n>