> 2.2.1 | Restore profile

> 2.2.1.1 | Description

> This chapter describes all the steps required to restore a profile. Two profiles are supported. First, use AT&V to check which profile is currently active. Depending on the result, you can enter AT&F to recall the factory settings or ATZ to restore the user profile saved with AT&W.

> 2.2.1.2 | Used AT commands

> Command | Explanation
> AT&V | Display the current configuration
> AT&F | Set all current parameters to manufacturer defaults
> ATZ | Set all current parameters to user defined profile

> For further details about the commands see [2].

> 2.2.1.3 | Flow chart

> Figure 5: Restore profile

> 2.2.1.4 | Hints

> Restoring a profile is possible at any time.

> 2.2.1.5 | Example

> ***************************************
> Comment: Restore profile
> ***************************************
> ***************************************
> Comment: Display current configuration
> ***************************************
> Subscr 1 Send: AT&V
> Subscr 1 Receive: AT&V
> Subscr 1 Receive: ACTIVE PROFILE:
> Subscr 1 Receive: E1 Q0 V1 X4 &C1 &D2 &S0 \Q0
> Subscr 1 Receive: S0:000 S3:013 S4:010 S5:008 S6:000 S7:060 S8:000 S10:002 S18:000
> Subscr 1 Receive: +CBST: 7,0,1
> Subscr 1 Receive: +CRLP: 61,61,78,6
> Subscr 1 Receive: +CR: 0
> Subscr 1 Receive: +FCLASS: 0
> Subscr 1 Receive: +ILRR: 0
> Subscr 1 Receive: +IPR: 0
> Subscr 1 Receive: +CMEE: 2
> Subscr 1 Receive: ^SCKS: 0,1
> Subscr 1 Receive: +CGSMS: 3
> Subscr 1 Receive:
> Subscr 1 Receive: OK
> ***************************************
> Comment: Restore manufacture defaults
> ***************************************
> Subscr 1 Send: AT&F
> Subscr 1 Receive: AT&F
> Subscr 1 Receive: OK
> ***************************************
> Comment: Display current configuration
> ***************************************
> Subscr 1 Send: AT&V
> Subscr 1 Receive: AT&V
> Subscr 1 Receive: ACTIVE PROFILE:
> Subscr 1 Receive: E1 Q0 V1 X4 &C1 &D2 &S0 \Q0
> Subscr 1 Receive: S0:000 S3:013 S4:010 S5:008 S6:000 S7:060 S8:000 S10:002 S18:000
> Subscr 1 Receive: +CBST: 7,0,1
> Subscr 1 Receive: +CRLP: 61,61,78,6
> Subscr 1 Receive: +CR: 0
> Subscr 1 Receive: +FCLASS: 0
> Subscr 1 Receive: +ILRR: 0
> Subscr 1 Receive: +IPR: 0
> Subscr 1 Receive: +CMEE: 0
> Subscr 1 Receive: ^SCKS: 0,1
> Subscr 1 Receive: +CGSMS: 3
> Subscr 1 Receive:
> Subscr 1 Receive: OK