Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| IM Profile
PREV NEXT | FRAMES NO FRAMES

## Uses of Package
com.siemens.icm.io

Packages that use com.siemens.icm.io
com.siemens.icm.io | Siemens IMP utility classes for accessing the functionality of a wireless module.

Classes in com.siemens.icm.io used by com.siemens.icm.io
ATCommandFailedException Signals that a requested device access via the ATCommand class failed.
ATCommandListener The ATCommandListener interface defines the capabilities for receiving unsolicited AT-Events (e.g. like "RING") and changes of the relevant incoming interface signals (RING, DCD and DSR).
ATCommandResponseListener The ATCommandResponseListenerListener interface defines the capabilities for receiving the response of sending an AT command to a module's AT interpreter.
BearerControlListener The BearerControlListener interface defines the capabilities for receiving bearer (e.g.
CommConnectionControlLinesListener The CommConnectionControlLinesListener interface defines the capability for receiving state changes of the DTR signal.
InPortListener The InPortListener interface defines the capabilities for receiving value changes at the input ports of the general purpose IO driver (GPIO).
LimitPulseCounterListener The LimitPulseCounterListener interface defines the capabilities for receiving the indication of a LimitPulseCounter when it has completed counting its number of pulses.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| IM Profile
PREV NEXT | FRAMES NO FRAMES

Submit a comment or suggestion Version 2.0 of IM Profile Specification
Java is a trademark or registered trademark of Sun Microsystems, Inc. in the US and other countries. Copyright (c) 1993-2002 Sun Microsystems, Inc. 901 San Antonio Road,Palo Alto, California, 94303, U.S.A. All Rights Reserved.