Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| IM Profile
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
com.siemens.icm.io.ATCommandFailedException

Packages that use ATCommandFailedException
com.siemens.icm.io | Siemens IMP utility classes for accessing the functionality of a wireless module.

Uses of ATCommandFailedException in com.siemens.icm.io

Methods in com.siemens.icm.io that throw ATCommandFailedException
`void` | `ATCommand.release()` Release resources locked by the ATCommand class.
`String` | `ATCommand.send(String ATCmd)` Send an AT command to the device.
`void` | `ATCommand.send(String ATCmd, ATCommandResponseListener response)` Send an AT command to the device.
`void` | `ATCommand.cancelCommand()` Cancel a running AT command.
`void` | `ATCommand.setDTR(boolean SignalState)` Set the state of the DTR (Data Terminal Ready) signal of the devices AT channel.
`boolean` | `ATCommand.getRING()` Get the state of the RING signal of the devices AT channel.
`boolean` | `ATCommand.getDCD()` Get the state of the DCD (Data Carrier Detect) signal of the devices AT channel.
`boolean` | `ATCommand.getDSR()` Get the state of the DSR (Data Set Ready) signal of the devices AT channel.
`boolean` | `ATCommand.getCONN()` Get the state of a data connection of the devices AT channel.

Constructors in com.siemens.icm.io that throw ATCommandFailedException
`ATCommand(boolean csdSupport)` Creates a new instance of the ATCommand class.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| IM Profile
PREV NEXT | FRAMES NO FRAMES

Submit a comment or suggestion Version 2.0 of IM Profile Specification
Java is a trademark or registered trademark of Sun Microsystems, Inc. in the US and other countries. Copyright (c) 1993-2002 Sun Microsystems, Inc. 901 San Antonio Road,Palo Alto, California, 94303, U.S.A. All Rights Reserved.